<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;"># This is a makemhr HRIR definition file.  It is used to define the layout and
# source data to be processed into an OpenAL Soft compatible HRTF.
#
# This definition is used to transform the near-field KEMAR HRIRs provided by
# Bosun Xie &lt;phbsxie@scut.edu.cn&gt; of the South China University of
# Technology, Guangzhou, China; and converted from SCUT to SOFA format by
# Piotr Majdak &lt;piotr@majdak.com&gt; of the Acoustics Research Institute,
# Austrian Academy of Sciences.
#
# A copy of the data (SCUT_KEMAR_radius_all.sofa) is available from:
#
#  http://sofacoustics.org/data/database/scut/SCUT_KEMAR_radius_all.sofa
#
# It is provided under the Creative Commons CC 3.0 BY-SA-NC license:
#
#  https://creativecommons.org/licenses/by-nc-sa/3.0/

rate     = 44100

# While the SOFA file is stereo, doubling the size of the data set will cause
# the utility to exhaust its address space if compiled 32-bit.  Since the
# dummy head is symmetric, the same results (ignoring variations caused by
# measurement error) can be obtained using mono channel processing.
type     = mono

points   = 512

radius   = 0.09

# This data set has 10 fields ranging from 0.2m to 1m.  The layout was
# obtained using the sofa-info utility.
distance = 0.2, 0.25, 0.3, 0.4, 0.5, 0.6, 0.7, 0.8, 0.9, 1.0

azimuths = 1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1;
           1, 24, 36, 72, 72, 72, 72, 72, 72, 72, 36, 24, 1

# Given the above compatible layout, we can automatically process the entire
# data set.
[ * ] = sofa : "./SCUT_KEMAR_radius_all.sofa" mono

</pre></body></html>